**PT**

**--Step 1**

Receive: 1>>{MAC/SN de L10},{HostName},{GroupName},#

Receive: 1>>20EFBDF5A3B9,BR1CNRKPT3,PT,#

**PASS**

Send: 1>>SERIALNO={SN},PNNAME={PN},#OK,UNIT STATUS IS VALID

Send: 1>>SERIALNO=20EFBDF5A3B9,PNNAME=RU9026000643#OK,UNIT STATUS IS VALID

**FAIL**

Send: 1>>SERIALNO={SN},PNNAME={PN},#{mensagem de erro do webservice}

Send: 1>>SERIALNO=20EFBDF5A3B9,PNNAME=RU9026000643#{mensagem de erro do webservice}

**--Step2**

**PASS**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#PASS

Receive: 2>>20EFBDF5A3B9;CSN=S00R419TECF5,CESN=X00400ETECF5,#PASS

Send: 2>>SERIALNO={SN}#OK,UNIT PASS!

Send: 2>>SERIALNO=20EFBDF5A3B9#OK,UNIT PASS!

**FAIL**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#{Error Description}

Receive: 2>>20EFBDF5A3B9;CSN=S00R419TECF5,CESN=X00400ETECF5,#Check temp fail

Send: 2>>SERIALNO={SN}#{Error Description}

Send: 2>>SERIALNO=20EFBDF5A3B9#Check temp fail

/\* ------------------------------------------------------------------------------------------------------- \*/

**FT**

**--Step 1**

Receive: 1>>{MAC/SN de L10},{HostName},{GroupName},#

Receive: 1>>20EFBDF5A3BB,BR1CNRKFT2,FT,#

**PASS**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#OK,UNIT STATUS IS VALID

Send: 1>>SERIALNO=20EFBDF5A3BB,CSN=S00R419H4JWE,CESN=X00400WH4JWE,PNNAME=RU9026000643#OK,UNIT STATUS IS VALID

**FAIL**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#{mensagem de erro do webservice}

Send: 1>>SERIALNO=20EFBDF5A3BB,CSN=S00R419H4JWE,CESN=X00400WH4JWE,PNNAME=RU9026000643#{mensagem de erro do webservice}

**--Step 2**

**PASS**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#PASS

Receive: 2>>20EFBDF5A3BB;CSN=S00R419H4JWE,CESN=X00400WH4JWE,#PASS

Send: 2>>SERIALNO={SN}#OK,UNIT PASS!

Send: 2>>SERIALNO=20EFBDF5A3BB#OK,UNIT PASS!

**FAIL**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#{Error Description}

Receive: 2>>20EFBDF5A3BB;CSN=S00R419H4JWE,CESN=X00400WH4JWE,#Check temp fail

Send: 2>>SERIALNO={SN}#{Error Description}

Send: 2>>SERIALNO=20EFBDF5A3BB#Check temp fail

/\* ------------------------------------------------------------------------------------------------------- \*/

**RC**

**--Step 1**

Receive: 1>>{MAC/SN de L10},{HostName},{GroupName},#

Receive: 1>>20EFBDF5A3B5,BR1CNRKRC4,RC,#

**PASS**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#OK,UNIT STATUS IS VALID

Send: 1>>SERIALNO=20EFBDF5A3B5,CSN=S00R419DE2RH,CESN=X00400UDE2RH,PNNAME=RU9026000643#OK,UNIT STATUS IS VALID

**FAIL**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#{mensagem de erro do webservice}

Send: 1>>SERIALNO=20EFBDF5A3B5,CSN=S00R419DE2RH,CESN=X00400UDE2RH,PNNAME=RU9026000643#{mensagem de erro do webservice}

**--Step 2**

**PASS**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#PASS

Receive: 2>>20EFBDF5A3B5;CSN=S00R419DE2RH,CESN=X00400UDE2RH,#PASS

Send: 2>>SERIALNO={SN}#OK,UNIT PASS!

Send: 2>>SERIALNO=20EFBDF5A3B5#OK,UNIT PASS!

**FAIL**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#{Error Description}

Receive: 2>>20EFBDF5A3B5;CSN=S00R419DE2RH,CESN=X00400UDE2RH,#Check temp fail

Send: 2>>SERIALNO={SN}#{Error Description}

Send: 2>>SERIALNO=20EFBDF5A3B5#Check temp fail

/\* ------------------------------------------------------------------------------------------------------- \*/

**LASER**

**--Step 1**

Receive: 1>>{MAC/SN de L10},{HostName},{GroupName},#

Receive: 1>>20EFBDF5A3B2,BR1CNRKLASER,LASER,#

**PASS**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#OK,UNIT STATUS IS VALID

Send: 1>>SERIALNO=20EFBDF5A3B2,CSN=S00R41913M8L,CESN=X00400Y13M8L,PNNAME=RU9026000643#OK,UNIT STATUS IS VALID

**FAIL**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#{mensagem de erro do webservice}

Send: 1>>SERIALNO=20EFBDF5A3B2,CSN=S00R41913M8L,CESN=X00400Y13M8L,PNNAME=RU9026000643#{mensagem de erro do webservice}

**--Step 2**

**PASS**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#PASS

Receive: 2>>20EFBDF5A3B2;CSN=S00R41913M8L,CESN=X00400Y13M8L,#PASS

Send: 2>>SERIALNO={SN}#OK,UNIT PASS!

Send: 2>>SERIALNO=20EFBDF5A3B2#OK,UNIT PASS!

**FAIL**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#{Error Description}

Receive: 2>>20EFBDF5A3B2;CSN=S00R41913M8L,CESN=X00400Y13M8L,#Check temp fail

Send: 2>>SERIALNO={SN}#{Error Description}

Send: 2>>SERIALNO=20EFBDF5A3B2#Check temp fail

/\* ------------------------------------------------------------------------------------------------------- \*/

**AUTO\_OBA**

**--Step 1**

Receive: 1>>{MAC/SN de L10},{HostName},{GroupName},#

Receive: 1>>20EFBDF5A4CC,BR1CNRKOBA1,OBA,#

**PASS**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#OK,UNIT STATUS IS VALID

Send: 1>>SERIALNO=20EFBDF5A4CC,CSN=S00R4199HAP9,CESN=X00400X9HAP9,PNNAME=RU9026000643#OK,UNIT STATUS IS VALID

**FAIL**

Send: 1>>SERIALNO={SN},CSN={CSN},CESN={CESN},PNNAME={PN}#{mensagem de erro do webservice}

Send: 1>>SERIALNO=20EFBDF5A4CC,CSN=S00R4199HAP9,CESN=X00400X9HAP9,PNNAME=RU9026000643#{mensagem de erro do webservice}

**--Step 2**

**PASS**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#PASS

Receive: 2>>20EFBDF5A4CC;CSN=S00R4199HAP9,CESN=X00400X9HAP9,#PASS

Send: 2>>SERIALNO={SN}#OK,UNIT PASS!

Send: 2>>SERIALNO=20EFBDF5A4CC#OK,UNIT PASS!

**FAIL**

Receive: 2>>{SN};CSN={CSN},CESN={CESN},#{Error Description}

Receive: 2>>20EFBDF5A4CC;CSN=S00R4199HAP9,CESN=X00400X9HAP9,#Check temp fail

Send: 2>>SERIALNO={SN}#{Error Description}

Send: 2>>SERIALNO=20EFBDF5A4CC#Check temp fail